**Lot 11 Watershed Electrofishing Report**

Date: Oct 11th, 2024

Time: 9:45 am

Location: Foxley River East

GPS Start: N: 46.68103ᵒ W: -64.00078ᵒ

GPS End: N: 46.68145ᵒ W: -64.00072ᵒ

The reach started at the GPS coordinates noted above. The 4ft culvert was the start hydraulic mark, however, net was placed at the beginning of stream past the sediment trap and another net was placed at the end GPS coordinate. The weather was overcast and windy at 12ᵒC. The water level at the time was very low which may have had an effect on the end results. No salmon were noted in any of the passes.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | First Pass | | Second Pass | | Third Pass | |
| Trout | Salmon | Trout | Salmon | Trout | Salmon |
| 1 | 10” | 0 | 5” | 0 | 7” | 0 |
| 2 | 12.5” |  | 7.3” |  | 9.3” |  |
| 3 | 5” |  | 6.3” |  | 3.5” |  |
| 4 | 7.2” |  | 7” |  | 4.6” |  |
| 5 | 5.5” |  | 3.5” |  |  |  |
| 6 | 8” |  | 4” |  |  |  |
| 7 | 9.3” |  | 4.5” |  |  |  |
| 8 | 7.1” |  | 9.2” |  |  |  |
| 9 | 6” |  | 5.5” |  |  |  |
| 10 | 4.5” |  | 9.3” |  |  |  |
| 11 | 5” |  | 5” |  |  |  |
| 12 | 6.3” |  | 7” |  |  |  |
| 13 | 4.6” |  |  |  |  |  |
| 14 | 7” |  |  |  |  |  |
| 15 | 9.2” |  |  |  |  |  |
| 16 | 9.5” |  |  |  |  |  |
| 17 | 8” |  |  |  |  |  |
| 18 | 3.5” |  |  |  |  |  |
| 19 | 4.5” |  |  |  |  |  |
| 20 | 6” |  |  |  |  |  |
| 21 | 7” |  |  |  |  |  |
| 22 | 9” |  |  |  |  |  |
| 23 | 6.5” |  |  |  |  |  |
| 24 | 7” |  |  |  |  |  |
| 25 | 5” |  |  |  |  |  |
| 26 | 8” |  |  |  |  |  |